
ADT835 Firmware Update Instruction

1. Copy the 835 firmware update package into the root directory of a flush memory disk;
2. Insert flush memory disk into 835 as pic.1;




Pic. 1

1. Select "Menu", then "Setup"




Pic. 2

1. Select "System Services"




Pic. 3

1. Select "System Update"



Pic. 4

1. Select "U-Disk Upgrade ", and confirm



Pic. 5

1. The updating process will run automatically,“Update Information” will display during the updating process. Reboot the 835 is the last step for firmware update.